digital_output group

This group contains all digital output signals.

Each signal is a sub group with the signal name as the group name.

"digital_output": {
"green_led": {
"type": "push pull"
"pad": "PA3"
}
}

type

defines what type of output mode should be used. Type can be:

push pull

open drain

type: enum

default: push pull

pad

defines the chip pad that the signal should be output on.

type: string

default: no default possible

invert

If this setting is set to “on” then turning this output “on” will generate a Low (Gnd) signal. Turning it “off” will generate a High (Vcc) level.

If this setting is set to “off” (=default) then turning this output “on” will generate a High (Vcc) signal. Turning it “off” will generate a Low (Gnd) level.

type: string

default: “off”