EZ-USB FX2G3

USB 2.0 @ 480MHz (High Speed)

Package: 104 LGA

Temperaure range: -45 .. 85 °C

GPIF/FIFO 16bit

Variants

part #	MCU	SRAM	Flash	SCB #	Peripherals
CYUSB2315-BF104AXI(T)	M0+	512 KB	256 KB	1	I2C
CYUSB2316-BF104AXI(T)	M0+	512 KB	256 KB	3	I2C, SPI, CAN
CYUSB2317-BF104AXI(T)	M0+	512 KB	512 KB	6	I2C, SPI, CAN, QSPI
CYUSB2318-BF104AXI(T)	M4/M0+	1024 KB	512 KB	6	I2C, SPI, CAN, QSPI, Crypto

Pins

ePad

A1..A56

B1..B48

abbreviation dictionary

abbreviation	long version	comment
DNU	Do not use	Do not use these connections for PCB signal routing channels. Do not connect any host system signal to these connections.
NC	Not connected	The connection may safely be used for routing space for a signal on a PCB. However, any signal connected to an NC pin must not have voltage levels higher than VIO.
RFU	Reserved for Future use	Do not use RFU connectors for PCB routing channels so that the PCB may take advantage of future enhanced features in devices with a compatible footprint.
SCB	Serial Control Block	A peripheral that can be used as I2C, UART or SPI