clock group

configuration of the used clocks.

"clock": {
"cpu": {
"source" : "hse",
"frequency" : "12 MHz",
}
}

source

defines the source of the clock signal. Supported clock sources are:

“hse” (High speed external)

…

type: enum

default: no default possible

frequency

defines the frequency that this clock has.

type: string (Hz, kHz, MHz)

default: “1 MHz”